     ----------------------------------------------------------------
      CARDS.TXT for Toshiba Card Manager Version 3.0  March 21, 1994
     ----------------------------------------------------------------

The following is a list of PCMCIA cards supported by the Toshiba Card
Manager Version 3.0

-------------------
- Data/Fax Modems -
-------------------
 AMT Starcard 2442
 Angia 14.4 type 3+ (16mm)
 Angia 14.4 type 2 (5mm)
 AT&T Paradyne
 ATI 14.4
 CP+ 24/96 PCM2496-1
 DataTrek 14.4
 EXP Thinfax 14.4/14.4
 EXP Thinfax 24/96
 E-Tech C1414X
 E-Tech C9624RX
 IBM 24/94 Fax Modem
 IBM Data/Fax 14.4/14.4
 Intel 96/96
 Intel ExCA 24/96 (iNC210US)
 Intel ExCA 2400+ (iNC110US)
 Intel ExCA 14.4
 Intel Satisfaxtion 14.4 (iNC230US)
 Megahertz 14.4/14.4 (non-XJack)
 Megahertz 14.4/14.4 XJack
 Megahertz 24/96 XJack
 MultiTech MT1432LT v.32bis
 Noteworthy T144NW (T144P/F)
 Noteworthy T24NW (T24P/F)
 PureData 14.4
 TDK DF2496A Fax Modem
 Toshiba T144PF4 
 Toshiba Canada Limited 14.4 (BC14400)

-------------------
- Lan             - 
-------------------
Note: Tested under a Novell Netware 3.11 environment:

  Model (Settings Used)
  3COM 3C589  {Tested with v1.0 of 3C589.COM}
	(MEM:D400-D7FF / IRQ: 9 / IO: 300)
  D-Link DE650
	(MEM:D000-D0FF / IRQ: 5 / IO: 300)
  IBM Ethernet  
	(MEM:D000-D3FF / IRQ: 5 / IO: 300)
  IBM Token Ring
	(MEM1:D800-DBFF / MEM2:D000-D1FF / IRQ: 9 / IO: A20-A23)
  Intel Ethernet iNC301 {Tested with CCMGR v2.00j}
	(MEM:D400-D7FF / IRQ: 5 / IO: 300)
  Kingston Ethernet (IBM)
	(MEM:D000-D3FF / IRQ: 5 / IO: 300)
  Magic RAM Ethernet (IBM)
	(MEM:D000-D3FF / IRQ: 5 / IO: 300)
  Magic RAM Token 16/4 (IBM)
	(MEM1:D800-DBFF / MEM2:D000-D1FF / IRQ: 9 / IO: A20-A23)
  National NE4100
	(MEM:D000-D3FF / IRQ: 5 / IO: 300)
  New Media Ethernet
	(MEM:D400-D7FF / IRQ: 5 / IO: 300)
  NoteWorthy Ethernet (IBM)
	(MEM:D000-D3FF / IRQ: 5 / IO: 300)
  NoteWorthy Token Ring (IBM)
	(MEM1:D800-DBFF / MEM2:D000-D1FF / IRQ: 9 / IO: A20-A23)
  PureData Ethernet (IBM)
	(MEM:D000-D3FF / IRQ: 5 / IO: 300)
  PureData Token Ring (IBM)
	(MEM1:D800-DBFF / MEM2:D000-D1FF / IRQ: 9 / IO: A20-A23)
  Socket Ethernet {Tested with SOCKETEA.COM v2.56}
	(IRQ: 5 / IO: 300)
  Thomas Conrad Ethernet (IBM)
	(MEM:D000-D3FF / IRQ: 5 / IO: 300)
  Thomas Conrad Token Ring (IBM)
	(MEM1:D800-DBFF / MEM2:D000-D1FF / IRQ: 9 / IO: A20-A23)
  Xircom Token Ring {Recomment using XIRCOM's enabler to configure card
		     instead of Card Manager if used in SLOT 1}
	(MEM1: D000-D1FF / IRQ: 5 / IO: 320)
  Xircom Ethernet {Recommend using Xircom's enabler to configure a card 
		   instead of Card Manager is used in SLOT 1}
	(MEM:D000-D3FF / IRQ: 5 / IO:  300)
       
-------------------
- Host Emulators  - 
-------------------
  IBM 3270
	(MEM1: CE00-D1FF / IRQ: 9 / IO: 2D0-2DF)
  IBM 5250
	{Although it is supported by Card Manager, the 5250 installation program
	 requests the IBM 5250 enabler during install.  Use IBM enabler.        }

-------------------
- ATA             -
-------------------
 Calluna 80Mb CT85MC
 Integral 85Mb 1882PA
 Integral 105Mb 8105PA
 Ministor 42Mb MP42P
 Ministor 85Mb MP85P
 Ministor 130Mb MP130P
 Maxtor 105Mb
 NoteWorthy 105Mb
 Sundisk 12V 20Mb
 Sundisk 5V 20Mb
 Sundisk 5V 10Mb
 Sundisk 12V 5Mb
 Sundisk 5V 5Mb
 Western Digital Caviar 40mb
 Hewlett-Packard Kittyhawk 20mb                  

-------------------
- Flash           -
-------------------
 AMD 1MB
 Intel Series I 1Mb      
 Intel Series I 2Mb
 Intel Series II 4Mb       
 Intel Series II 2Mb
 Intel Series II 10Mb      

-------------------
- SRAM            -
-------------------
 New Media 2MB SRAM

-------------------
- Misc            -
-------------------
 Adaptec SlimSCSI
 New Media Visual SCSI
 New Media Bus Toaster SCSI
 Socket Communications Serial I/O Adapter
	

