      ------------------------------------------------------------------
       REMOVE.TXT for Toshiba Card Manager Version 3.0 - March 21, 1994
      ------------------------------------------------------------------

The following discussion gives general guidelines on how to remove the        
previous (rev 1.0) version of Toshiba Card Manager, and the Toshiba
PCMCIA.SYS Enabler (if installed), both of which should be done prior 
to installing Toshiba Card Manager version 3.0.

How to remark out lines in different files:
  
In DOS files (CONFIG.SYS and AUTOEXEC.BAT), just add the word REM at 
the beginning of the line you wish to remark out.
  
In Windows files (WIN.INI and SYSTEM.INI), just add a semicolon to
the beginning of the line you wish to remark out.


Removing Toshiba Card Manager Version 1.0:

The CONFIG.SYS File:

1. Locate the Toshiba Card Manager drivers within CONFIG.SYS, and delete 
   or remark out the "device=" or "devicehigh=" lines which include them.
   The drivers are:
     PCMSS.EXE
     PCMCS.EXE
     PCMSCD.EXE
     PCMATA.SYS
     PCMFFCS.EXE
     MSFLASH.SYS
     DBLFLASH.EXE
  
2. Locate any added EMM386 excludes for Toshiba Card Manager and remove
   these from the "device=emm386.exe" line.  These excludes are of the
   form "X=nnnn-nnnn". If you are using a different memory manager such 
   as QEMM or 386MAX, please refer to your documentation for the exact
   syntax of the Exclude parameters for these utilities.



The AUTOEXEC.BAT File

1. Locate any PATH statements which include the Toshiba Card Manager 
   directory, and delete that directory from the statement. 
   
2. Locate any path statement that appends the Toshiba Card Manager
   path to the system path, and delete or remark it out.
   E.g., "PATH = %PATH%;C:\PCMPLUS"
   


The Windows File WIN.INI

1. Locate the [windows] section and remove PCMWARN.EXE from the "run=" line.



The Windows File SYSTEM.INI

1. Locate the [386Enh] section.  Within this section, modify the 
   following lines:

     device=pcmvcd.386    - delete or remark it out.

     ;device=*vcd.386     - remove the leading semicolon, which will
			    "un-remark the line". 
			    
     any "EMMExclude=" lines containing address ranges which match 
     the ranges in the "device=emm386.exe" line in CONFIG.SYS.  
     Delete or remark out such EMMExclude lines.

     any "PCMCIAComx=" statements.  Delete or remark them out.

     any "COMxBASE=" statements appearing between the "patched by PCM+"
     statements/remarks.  Delete or remark them out.


2. Locate and delete or remark out the entire [PCMCIA] section, if present.

3. Do not modify or delete any other lines in SYSTEM.INI




Removing the Toshiba PCMCIA.SYS Enabler:

1. Remove or remark out any lines in CONFIG.SYS containing the text 
   strings "PCMCIA.SYS" or "PCMCIA2.SYS".

2. Remove any "X=nnnn-nnnn" parameters in the CONFIG.SYS 
   "device=EMM386.EXE" line which may have been added to support
   PCMCIA.SYS or PCMCIA2.SYS.




After All Modifications Are Made

1. Reboot the system.  This makes all of the changes effective.

2. Continue with your installation of Toshiba Card Manager Version 3.0.

